**INSTRUCTIONS FOR THE GLASS WASHER**

**TO TURN ON**

1 MAKE SURE THE SWITCH IS ON, BOTTOM LEFT ON THE WALL

2 REPLACE THE DRAIN PLUG IN THE CENTER OF THE DRAIN AND

 TURN CLOCKWISE TO SECURE.

3 CLOSE THE DOOR AND PRESS THE LEFT-HAND BUTTON WHICH WILL SWITCH ON THE MACHINE. THE WATER WILL ENTER AUTOMATICALLY, IT TAKES APROXIMAETELY 15 MINUTES TO REACH WORKING TEMPERATURE.

4 KEEP THE LOADING TRAY OVER THE DRAINING BOARD NEXT TO THE SINK ANY HEAVILY SOILED GLASSES E.G. FRUIT JUICE, GUINNESS, OR COFFEE CUPS SHOULD BE RINSED WELL BEFORE BEING PUT IN THE TRAY.

5 AFTER LOADING THE TRAY INTO THE MACHINE CLOSE THE DOOR AND PRESS THE RIGHT-HAND BUTTON AND THE WASH CYCLE WILL START. EACH WASH CYCLE TAKES ABOUT 2 MINUTES.

6 USE A **CLEAN** TEATOWEL TO POLISH THE RIM OF THE GLASSES BEFORE PUTTING AWAY. Sometimes it is necessary to rewash especially if there is a heavy deposit of lipstick., or fruit juice, or coffee.

**TO DRAIN THE MACHINE**

1 REMOVE THE TRAY, TAKE OUT THE CENTRAL PLUG IN THE DRAIN BY TURNING ANTI CLOCKWISE ½ TURN, REMOVE COMPLETELY AND LEAVE ON THE DRAINING BOARD.

2 CLOSE THE DOOR AND PRESS THE LEFT BUTTON, which seems strange because it’s the on/off button however., HOLD THE BUTTON SECOND FROM THE LEFT UNTILL YOU HEAR THE MACHINE START TO DRAIN.

3 ONCE THE MACHINE HAS DRAINED SWITCH OFF AT THE MAIN SWITCH.